- 0

# 900

#900, Lyptus, "F"

- Description
- More Details
- Specifications

##

Door shown in Lyptus (Lyptus wood is currently unavailable) with outside edge profile "F"

- Series 900 doors are constructed of 100% solid wood
- The natural range of colors allowed in all wood species including limited amounts of sap and mineral streaks
- "SELECT" woods are available in most woods for a higher grade of color and grain match (Select White Pine only available with a solid panel.) “PREMIUM” woods are available for some woods, center panels have to be upgraded to solid wood. See Wood Species for details of Select and Premium grades.
- Series 900 doors have 13/16" thick frames, 5/4 (1") thick frames available for most woods
- OPTIONAL square/round pegs can be added to the corners of most door styles doors, see Door Options
- Standard outside edge profiles “A” through “M” are available for 900 series doors

Panel and inside frame detail

Outside edge profile F shown on door

Line drawing of #900 door

Stile Width: | 2-3/8"
Rail Width: | 2-3/8"
Minimum Door Size* (WxH): | 7-5/8" x 7-5/8"
Minimum Trimmed Door Size* (WxH): | 5-7/8" x 5-7/8"
Maximum Door Size (WxH): | 26" x 96"
Extra Center Rail Required At: | 48"
Drawer Front Compliments This Door: | #500 and #590
Glass or Open Frame Door Available: | Yes
Waterfall Frame Thickness: | This frame style cannot be ordered less than 13/16" thick
* | If one minimum is used from above specs, add 2" to other

!
Mobile mode
To create online store ShopFactory eCommerce software was used.