- 0

# 255

- Description
- More Details
- Specifications

##

Door shown in Select Maple with Black Walnut Stripe Pattern and "A" profile

- Construction is a solid wood slab
- Drawer front style #500 compliments this door
- Glass or open frame door is NOT available
- Two battens on the back side of the door are 5/8" thick by 1-5/8" wide located 2" from the side edge and 3" from the top and bottom
- A 3rd batten is required past 48" in height, a 4th batten past 66" in height
- Matching drawer front has horizontal grain with accent strips from the top down
- Door has accent stripes as follows: 2" wide main wood choice, 3/8" wide accent wood choice, 3/8" wide main wood choice, 3/4" side accent wood choice with the balance the main wood choice.
- Matching drawer front has horizontal grain with accent stripes from the top down as follows: 1-1/2" main wood, 3/8" accent wood, 3/8" main wood, 3/4" accent wood with the remaining width the main wood. Minimum height for this drawer front is 4".

Cross-Section Detail

Outside edge profile C shown on door

Line drawing of #255 door

Minimum Size | 5-1/2" x 4"
Minimum Trimmed Size | 5-1/2" x 4"
Maximum Size | 26" x 96"
Extra Center Rail Required At: | NA
Drawer Front Compliments This Door: | #500
Glass or Open Frame Door Available: | No

!
Mobile mode
To create online store ShopFactory eCommerce software was used.