- 0

# 212

Scherr's Cabinet & Doors 212 Style Doors. Shown here in Paint-Grade Poplar, painted Sherwin Williams' Dover White, and has an 'I' outside profile.

- Description
- More Details
- Specifications

##

Door shown in Paint Grade Poplar with outside edge profile 'M', painted Sherwin Williams' Dover White

• Series 212 doors are constructed of 100% solid wood
• The natural range of colors allowed in all wood species including limited amounts of sap and mineral streaks
• Select woods are available in most woods for a higher grade of color and grain match (Select White Pine only available with a 1/2" solid panel.) Premium woods are available for some woods, center panels have to be upgraded to solid wood. See Wood Species for details of Select and Premium grades.
• Series 212 doors have 13/16" thick frames, 5/4 (1") thick frames available for most woods
• OPTIONAL square/round pegs can be added to the corners of most door styles doors, see Door Options
• Standard outside edge profiles 'A' through 'M' are available for 212 series doors

Panel and inside frame detail

Outside edge profile M shown on door

Line drawing of #212 door

Stile Width: | 2/3/8"
Rail Width: | 2-3/8"
Center Stile Width: | 2-3/8"
Minimum Door Size* (WxH): | 13-1/8" x 7-3/4"
Minimum Trimmed Door Size* (WxH): | 10-1/2" x 6"
Maximum Door Size (WxH): | 26" x 96"
Extra Center Rail Required At: | 48"
Drawer Front Compliments This Door: | #500 and #520
Glass or Open Frame Door Available: | Yes
* | If one minimum is used from above specs, add 2" to other.

!
Mobile mode
To create online store ShopFactory eCommerce software was used.