- 0

# 412

Scherr's Cabinet & Doors 412 Style Doors. Shown here in Select Cherry with a 'K' outside profile.

- Description
- More Details
- Specifications

##

Door shown in Select Cherry with outside edge profile 'K'

• Series 400, 409, 412, 414, 415, 416, 475, 478, 490, 493, and 494 doors have solid wood frames with 1/4" plywood panels - a solid wood panel upgrade is available
• Series 491 and 492 doors have solid wood frames with 1/4" plywood panels (solid wood panel upgrade is NOT available because of corner blocks)
• Series 476 door is constructed of 100% solid wood
• The natural range of colors allowed in all wood species including limited amounts of sap and mineral streaks
• 'Select' woods are available in most woods for a higher grade of color and grain match (Select White Pine only available with 1/2” solid panel.) 'Premium' woods are available for some woods, center panels have to be upgraded to 1/2” solid wood. See Wood Species for details of 'Select' and 'Premium' grades.
• Series 400 doors have 13/16" thick frames, 5/4 (1") thick frames available for most woods
• Optional square/round pegs can be added to the corners of most door styles, see Door Options
• Standard outside edge profiles 'A' through 'M' are available for 400 series doors

Panel and inside frame detail

Outside edge profile K shown on door

Line drawing of #412 door

Stile Width: | 2/3/8"
Rail Width: | 2-3/8"
Center Stile Width: | 2-3/8"
Minimum Door Size* (WxH): | 11-1/8" x 7-3/4"
Minimum Trimmed Door Size* (WxH): | 8-1/2" x 6"
Maximum Door Size (WxH): | 26" x 96"
Extra Center Rail Required At: | 48"
Drawer Front Compliments This Door: | #500 and #540
Glass or Open Frame Door Available: | Yes
Solid Wood Panel Upgrade Available: | Yes
* | If one minimum is used from above specs, add 2" to other.

!
Mobile mode
To create online store ShopFactory eCommerce software was used.