- 0

# Red Oak Select

- Description

Select Red Oak will be selected for a higher grade of color and grain match with a moderate amount of color variation allowed between doors. Limited pin burls may be present and mineral stains no larger than 1/8" wide by 3" long. A small amount of sapwood may appear only in machined areas of panel and outside edge of frame.
!
Mobile mode
To create online store ShopFactory eCommerce software was used.