- 0

# 216

Scherr's Cabinet & Doors 216 Style Doors. Shown here in Clear White Pine with an 'F' outside profile.

- Description
- More Details
- Specifications

##

Door shown in Clear White Pine with outside edge profile 'F'

• Series 216 doors are constructed of 100% solid wood
• The natural range of colors allowed in all wood species including limited amounts of sap and mineral streaks
• Select woods are available in most woods for a higher grade of color and grain match (Select White Pine only available with a 1/2" solid panel.) Premium woods are available for some woods, center panels have to be upgraded to solid wood. See Wood Species for details of Select and Premium grades.
• Series 216 doors have 13/16" thick frames, 5/4 (1") thick frames available for most woods
• OPTIONAL square/round pegs can be added to the corners of most door styles doors, see Door Options
• Standard outside edge profiles 'A' through 'M' are available for 216 series doors

Panel and inside frame detail

Outside edge profile F shown on door

Line drawing of #216 door

Stile Width: | 2/3/8"
Rail Width: | 2-3/8"
Crossbar (Center Rail) Width: | 2-3/8"
Center Stile Width: | 2-3/8"
Minimum Door Size* (WxH): | 13-1/8" x 13-1/8"
Minimum Trimmed Door Size* (WxH): | 10-1/2" x 10-1/2"
Maximum Door Size (WxH): | 26" x 96"
Extra Center Rail Required At: | NA
Panel is Split: | Customer must specify top panel opening (distance between bottom edge of top rail and top edge of crossbar), if no opening is specified the default is 6".
Drawer Front Compliments This Door: | #500 and #520
Glass or Open Frame Door Available: | Yes
* | If one minimum is used from above specs, add 2" to other.

!
Mobile mode
To create online store ShopFactory eCommerce software was used.