- 0

# 214

Scherr's Cabinet & Doors 214 Style Doors. Shown here in Select Birch with a 'D' outside profile.

- Description
- More Details
- Specifications

##

Door shown in Select Birch with outside edge profile 'D'

• Series 214 doors are constructed of 100% solid wood
• The natural range of colors allowed in all wood species including limited amounts of sap and mineral streaks
• Select woods are available in most woods for a higher grade of color and grain match (Select White Pine only available with a 1/2" solid panel.) Premium woods are available for some woods, center panels have to be upgraded to solid wood. See Wood Species for details of Select and Premium grades.
• Series 214 doors have 13/16" thick frames, 5/4 (1") thick frames available for most woods
• OPTIONAL square/round pegs can be added to the corners of most door styles doors, see Door Options
• Standard outside edge profiles 'A' through 'M' are available for 214 series doors

Panel and inside frame detail

Outside edge profile D shown on door

Line drawing of #214 door

Stile Width: | 2/3/8"
Rail Width: | 2-3/8"
Crossbar (Center Rail) Width: | 2-3/8"
Center Stile Width: | 2-3/8"
Minimum Door Size* (WxH): | 13-1/8" x 13-1/8"
Minimum Trimmed Door Size* (WxH): | 10-1/2" x 10-1/2"
Maximum Door Size (WxH): | 26" x 96"
Extra Center Rail Required At: | NA
Panel is Split: | 50% bottom, 50% top and 50/50 side to side
Drawer Front Compliments This Door: | #500 and #520
Glass or Open Frame Door Available: | Yes
* | If one minimum is used from above specs, add 2" to other.

!
Mobile mode
To create online store ShopFactory eCommerce software was used.