- 0

# 700

Scherr's Cabinet & Doors 700 Style Doors. Shown here in Select Walnut with an 'A' outside profile.

- Description
- More Details
- Specifications

##

Door shown in Select Walnut with outside edge profile 'A'

• Series 700 doors have solid wood frames with 1/4" plywood panels - solid wood panel upgrade is available
• The natural range of colors allowed in all wood species including limited amounts of sap and mineral streaks
• 'Select' woods are available in most woods for a higher grade of color and grain match (Select White Pine only available with a 1/2" solid wood panel.) 'Premium' woods are available for some woods, center panels have to be upgraded to solid wood. See Wood Species for details of 'Select' and 'Premium' grades.
• Series 700 doors have 13/16" thick frames, 5/4 (1") thick frames available for most woods
• Optional square/round pegs can be added to the corners of most door styles doors, see Door Options
• Standard outside edge profiles 'A' through 'M' are available for 700 series doors

#700 Door Below in Paint Grade Poplar, "F" with 2 coats White Primer:

Panel and inside frame detail

Outside edge profile A shown on door

Line drawing of #700 door

Stile Width: | 2/3/8"
Rail Width: | 2-3/8"
Minimum Door Size* (WxH): | 6-1/2" x 6-1/2"
Minimum Trimmed Door Size* (WxH): | 4-3/4" x 4-3/4"
Maximum Door Size (WxH): | 26" x 96"
Extra Center Rail Required At: | 48"
Drawer Front Compliments This Door: | #500 and #570
Glass or Open Frame Door Available: | Yes
Solid Wood Panel Upgrade Available: | Yes
Waterfall Frame Thickness: | This frame style cannot be ordered less than 13/16" thick
* | If one minimum is used from above specs, add 2" to other.

!
Mobile mode
To create online store ShopFactory eCommerce software was used.