- 0

# 915

#915, Maple, "K"

- Description
- More Details
- Specifications

##

Door shown in Maple with outside edge profile "K"

• Series 915 doors are constructed of 100% solid wood
• The natural range of colors allowed in all wood species including limited amounts of sap and mineral streaks
• "SELECT" woods are available in most woods for a higher grade of color and grain match (Select White Pine only available with a solid panel.) “PREMIUM” woods are available for some woods, center panels have to be upgraded to solid wood. See Wood Species for details of Select and Premium grades.
• Series 915 doors have 13/16" thick frames, 5/4 (1") thick frames available for most woods
• OPTIONAL square/round pegs can be added to the corners of most door styles doors, see Door Options
• Standard outside edge profiles “A” through “M” are available for 915 series doors

Panel and inside frame detail

Outside edge profile K shown on door

Line drawing of #915 door

Stile Width: | 2-3/8"
Rail Width: | 2-3/8"
Minimum Door Size* (WxH): | 13" x 13"
Minimum Trimmed Door Size* (WxH): | 10-3/8" x 10-1/2"
Maximum Door Size (WxH): | 26" x 96"
Extra Center Rail Required At: | NA
Drawer Front Compliments This Door: | #500 and #590
Glass or Open Frame Door Available: | Yes
Center Rail Width: | 2-3/8"
Center Stile Width: | 2-3/8"
Waterfall Frame Thickness: | This frame style cannot be ordered less than 13/16" thick
* | If one minimum is used from above specs, add 2" to other
** | Top panel has horizontal wood grain and bottom two panels have vertical wood grain, unless specified otherwise
*** | Customer must specify top panel opening (distance between the top rail and center stile), if no opening is specified, the default will be 6"

!
Mobile mode
To create online store ShopFactory eCommerce software was used.