- 0

# 213

Scherr's Cabinet & Doors 213 Style Doors. Shown here in Hickory with a 'K' outside profile.

- Description
- More Details
- Specifications

Left hand door is shown in picture.

##

Door shown in Hickory with outside edge profile 'K'

• Series 213 doors are constructed of 100% solid wood
• The natural range of colors allowed in all wood species including limited amounts of sap and mineral streaks
• Select woods are available in most woods for a higher grade of color and grain match (Select White Pine only available with a 1/2" solid panel.) Premium woods are available for some woods, center panels have to be upgraded to solid wood. See Wood Species for details of Select and Premium grades.
• Series 213 doors have 13/16" thick frames, 5/4 (1") thick frames available for most woods
• OPTIONAL square/round pegs can be added to the corners of most door styles doors, see Door Options
• Standard outside edge profiles 'A' through 'M' are available for 213 series doors

Panel and inside frame detail

Outside edge profile K shown on door

Line drawing of #213 door

Stile Width: | 2/3/8"
Rail Width: | 2-3/8"
Crossbar (Center Rail) Width: | 2-3/8"
Center Stile Width: | 2-3/8"
Minimum Door Size* (WxH): | 13-1/8" x 15"
Minimum Trimmed Door Size* (WxH): | 10-1/2" x 12-3/8"
Maximum Door Size (WxH): | 26" x 96"
Extra Center Rail Required At: | NA
Panel is Split: | For left hand door (shown) the left panel is split 60% bottom / 40% top, the right panel is split 40% bottom / 60% top, a right hand door is opposite.
Drawer Front Compliments This Door: | #500 and #520
Glass or Open Frame Door Available: | Yes
* | If one minimum is used from above specs, add 2" to other.

!
Mobile mode
To create online store ShopFactory eCommerce software was used.