- 0

Cabinets Assembled By You™

Edge Banding

Edge Banding for the Front of Your Cabinets

The edge banding is the thin material that covers the front face of the cabinets utilizing frameless construction. Typically we will use edge banding that is made from the same material as the exterior of your cabinets. (i.e. If your cabinets are a walnut veneer, we will use edge banding made from real walnut to match.) Wood edge banding is made from real wood and can be stained, clear coated, or painted to blend nicely with any component of the cabinet. Every type of wood that you can have your cabinets made out of applies to our real wood edge tape selection as well.
You have the following options for edge banding:

- Wood edge banding to match the cabinet interior or exterior
- PVC edge banding to match the cabinet interior or exterior

NOTE: PVC is a vinyl banding which is available in many solid colors and wood grain patterns. Wood banding is the most common type used in kitchen cabinets but the PVC banding is more durable and can be used in commercial and other room applications of cabinetry.

Edge Banding Size/Thickness Standards:

- Cabinet edges get 0.5 mm (1/32 in) thick edge banding standard
- #125 Doors get 1.5 mm (3/32 in) thick edge banding standard *whenever available. If not, then 0.5 mm (1/32 in) thick edge banding.
- For refrigerator and appliance openings that are always exposed, we will use hardwood that is 5 mm thick (on the exposed edges only)
- Bookshelves, appliance cabinet floors, and some cabinet edges that require extra protection and durability will have hardwood attached in our shop (whenever possible with respect to shipping constraints) at a standard thickness of 13/16"
- Extra thick 3 mm PVC edge taping is available for extra durability (great for cabinets in garages, mudrooms, utility rooms, shops, etc.)

NOTE: Great care is taken to ensure that all cabinet components that receive edge banding will have the same final size in the end no matter how thick the edge banding. Cabinet components are cut with great precision to compensate for each size of edge taping. (i.e. If a cabinet component needs to be 24 inches exactly but has 1/32" edge-banding on its face, the component will be cut to 23 31/32". This way when the edge taping is applied it comes out to exactly the correct size!)

!
Mobile mode
To create online store ShopFactory eCommerce software was used.