- 0

Open Frame Doors & Mullion Grids

Open Frame Doors without the panel, prepared for square glass or insert (not included.) The following door styles are available.

| • Series 100 doors (100 - 118 plus 140) • Series 200 doors (200 - 218 plus 240) • Series 400 doors (400 - 416 and 475 - 495) • Series number 260 and 460 doors • Series 600 doors • Series 700 doors (700 - 718 plus 740) • Series 800 doors (800 - 818 plus 840) • Series 900 doors (900 - 918 plus 940) • The following doors do NOT have the open frame option available: Series number 125, 250 and 255.
Mullion Grid frames will be constructed with equally spaced lites. Custom spacing or an odd number of lites in a frame are available, attach a drawing to your order. Available in the listed above Frame Only Doors.
#700 Open Frame Walnut Door with 6-Lite Grid Shown | • Mullions for Series 100, 200 and 400 frame styles • Mullions for Series 700, 800 and 900 frame styles • Mullions are stationary and cannot be removed. The mullions are splined for added strength. • Mullions are 1" wide on #100 and #200 doors. • Mullions are 3/4" wide on #400 doors. • Mullions are 1-1/4" wide on #700, #800 and #900 doors. • Mullions for 600 series only for the doors 600, 602 and 604. • ALL designs (100 through 900) are prepared for a one piece square glass or insert (not included.)
| Inset Mullion Grids frames will be constructed with equally spaced lites. Custom spacing or an odd number of lites in a frame are available. Mullion Grid for Doors Series #475, 476, 478 and 494-SW frames.
| Glass Retainer, Vinyl or Wood An OPTIONAL Vinyl Glass Retainer molding or matching Wood Retainer is available to hold glass or insert into open frame doors.

!
Mobile mode
To create online store ShopFactory eCommerce software was used.