- 0

# 250

- Description
- More Details
- Specifications

##

Door shown in Lyptus with outside edge profile "A"

- Construction is a solid wood slab
- Drawer front style #500 compliments this door
- Glass or open frame door is NOT available
- Two Battens on the back side of the door are 5/8" thick by 1-5/8" wide located 2" from the side edge and 3" from the top and bottom. Battens are installed to help prevent/slow solid wood slab doors from naturally cupping over time.
- A 3rd Batten is required past 48" in height, a 4th batten past 66" in height
- Wood Species Available in:

- Ash
- Beech
- Birch (Standard or Select)
- Cherry (Standard, Select, or Rustic)
- Hickory
- Mahogany (Sapele)
- Maple (Paint-Grade, Standard, or Select)
- Poplar (Paint-Grade or Stain-Grade)
- Red Alder (Standard, Select, or Rustic)
- Red Oak (Standard, Select, Rustic, Rift-Sawn, or Quarter-Sawn)
- Walnut (Standard, Select, or Rustic)
- White Oak (Standard, Select, Rustic, Rift-Sawn, or Quarter-Sawn)

Cross-Section Detail

Outside edge profile C shown on door

Line Drawing of #250

Minimum Door Size* (WxH): | 4" x 4"
Minimum Trimmed Door Size* (WxH): | 4" x 4"
Maximum Door Size (WxH): | 26" x 96"
Extra Center Rail Required At: | NA
Drawer Front Compliments This Door: | #500
Glass or Open Frame Door Available: | No

!
Mobile mode
To create online store ShopFactory eCommerce software was used.