- 0

# 260

Scherr's Cabinet & Doors 260 Style Doors. Shown here in Rustic Red Alder with an 'I' outside profile.

- Description
- More Details
- Specifications

#260 Door Style has a "Traditional" panel profile instead of "Cove"

##

Door shown in Rustic Red Alder with outside edge profile 'I'

• Series 260 doors are constructed of 100% solid wood
• The natural range of colors allowed in all wood species including limited amounts of sap and mineral streaks
• Select woods are available in most woods for a higher grade of color and grain match. Premium woods are available for some woods. See Wood Species for details of Select and Premium grades.
• Series 260 doors have 13/16" thick frames, 5/4 (1") thick frames available for most woods
• OPTIONAL square/round pegs can be added to the corners of most door styles doors, see Door Options
• Standard outside edge profiles 'A' through 'M' are available for 260 series doors

• NOTE: this door has a different panel within the frame compared to the other 200 Series doors! See 'Panel & Inside Frame Detail' in the 'More Details' tab.

Panel and inside frame detail

Outside edge profile I shown on door

Line drawing of #260 door

Stile Width: | 2/3/8"
Rail Width: | 2-3/8"
Minimum Door Size* (WxH): | 7-3/4" x 7-3/4"
Minimum Trimmed Door Size* (WxH): | 6" x 6"
Maximum Door Size (WxH): | 26" x 96"
Extra Center Rail Required At: | 48"
Drawer Front Compliments This Door: | #500 and #526
Glass or Open Frame Door Available: | Yes
* | If one minimum is used from above specs, add 2" to other.

!
Mobile mode
To create online store ShopFactory eCommerce software was used.