- 0

# Calico Hickory

- Description

Face: “A” grade plain sliced heartwood and/or sapwood

Back: #2 grade heartwood and/or sapwood

Edge banding: Hickory

Characteristics: Ranges in color from white to creamy pinkish brown with dark streaks; veneer is random matched to achieve a “calico” appearance; pin knots are allowed, 1/8” maximum, blending color, with no more than 2 per square foot on face veneer and unlimited on back veneer.

!
Mobile mode
To create online store ShopFactory eCommerce software was used.