- 0

# Plain Sliced Alder

- Description

Face: “A” grade plain sliced heartwood

Back: #2 grade veneer; some sapwood acceptable

Edge banding: Alder

Characteristics: Pinkish-brown in color; veneer fine textured with a subdued grain pattern; pin knots are allowed, 1/8” maximum, blending color, with no more than 2 per square foot on face veneer and unlimited on back veneer.

!
Mobile mode
To create online store ShopFactory eCommerce software was used.