- 0

GIBRALTAR

BRAELYN

WEATHERED GREY OAK

PALOMINO

RUSTIC LIGHT OAK

NIZZA

SWISS ELM SKYE

### Authentic Texture

Unique, matte, woodgrain textures embossed into a membrane that is pressed over the face & sides of an engineered core providing stability and seamless, joint-free construction

### Tough

Scratch resistant and resilient, what little wear and tear that makes it into the face material is obscured by the natural wood-grain texture

### Versatile

Fillers, cover panels, molding & floating shelves are available to compliment your custom-sized doors and drawer fronts

Door Style | Slab
Construction | Membrane pressed face and sides with slight radius edges
Back Material | Standard back is White TFL (other options available)
Core | 3/4" engineered core (MDF)
Grain Direction | Vertical grain standard for doors. Horizontal grain standard for drawer fronts
Route for Glass | Standard route available
Minimum Size | 3" x 3" minimum
Maximum Size | 48" x 96" maximum, warranted to 31" x 60"

For warranty information on Engineered Doors from Northern Contours, click here

ENGINEERED DOORS ARE AVAILABLE FOR IKEA PROJECTS ONLY

### Weathered Grey Oak

### Rustic Light Oak

### Gibraltar

### Braelyn

### Palomino

### Nizza

### Swiss Elm Skye

!
Mobile mode
To create online store ShopFactory eCommerce software was used.