- 0

Center Panel Options

Solid Panel Upgrades for Plywood

An Optional 1/2" solid wood panel upgrade is available for several door styles listed below.

Available for door series 100-140 and 700-740 without arches. Also doors 400-416, 475, 478,490, 493 and 494 can upgrade to a solid panel.

Grooved Plywood Panels

Doors with plywood panels can get optional 'V'-groove or square cut grooves with a standard spacing of 1-1/2", *custom spacing is available.

'V'-Grooves in 1/4" Plywood Panel

Square-Cut Grooves in 1/4" Plywood Panel

Both styles available for door series 100-140, 700-740, 400-416, 475, 478, 493, and 494 with plywood panels. Note: Matching 5-piece drawer fronts are available with some restrictions.

Grooved or Beaded Solid Panels

Doors with solid wood panels can get optional 'V'-grooves or beaded grooves with a standard spacing of 1-1/2", *custom spacing is available.

Grooves in 1/2" Solid Panel

Beaded Grooves in 1/2" Solid Panel

Groves in Solid Raised Panel

Beaded Grooves in Solid Raised Panel

'V'-Grooves or Beaded Grooves are available for door series 200-240, 800-840, 900-940, 476, 260, and 460. The grooves are also available for doors with plywood panels that are upgraded to solid panels. Note: Matching 5-piece drawer fronts are available with some restrictions. All groove styles and panel types have a standard groove spacing of 1-1/2" on center. *Custom spacing is also available.

!
Mobile mode
To create online store ShopFactory eCommerce software was used.