- 0

# Scherr's Cabinet & Doors, Inc.

### Authentic Texture

Unique, matte, woodgrain textures embossed into a membrane that is pressed over the face & sides of an engineered core providing stability and seamless, joint-free construction

### Tough

Scratch resistant and resilient, what little wear and tear that makes it into the face material is obscured by the natural wood-grain texture

### Versatile

Fillers, cover panels, molding & floating shelves are available to compliment your custom-sized doors and drawer fronts

Door Style | Shaker
Construction | 5-piece Shaker, profile wrapped stiles and rails, membrane pressed flat insert panels
Back Material | Matches front
Core | 3/4" Engineered core (MDF)
Grain Direction | Vertical grain is standard on door insert panels, horizontal grain is standard on drawer front insert panels
Route for Glass | Available
Minimum Size | 7.6" x 6" (Frame and Panel) 3" x 3" (Slab)
Maximum Size | 37" x 96" (Warranted to 37" x 60")

For warranty information on Engineered Doors from Northern Contours, click here

ENGINEERED DOORS ARE AVAILABLE FOR IKEA PROJECTS ONLY

SAMPLES DOORS ARE NOT YET AVAILABLE, BUT WILL BE SOON!

### Weathered Grey Oak

### Rustic Light Oak

!
Mobile mode
To create online store ShopFactory eCommerce software was used.