- 0

ONYX

FLINT

GAUNTLET

SILT

HAZE

MIST

MIDNIGHT

SURF

DENIM

SAGE

ALOE

STRATUS

### Seamless

A durable, soft-touch membrane is pressed over the face & sides of an engineered core providing stability and seamless, joint-free construction

### Silky Texture

Paint-like, low-sheen & matte—but with an engineered edge. Durable and easy to clean with just soap and water

### Versatile

Fillers, cover panels, molding & floating shelves are available to compliment your custom-sized doors and drawer fronts

Door Style | Shaker Slim
Construction | Membrane pressed face and sides with slight radius edges
Back Material | Standard back is White TFL (Other options available)
Core | 3/4" Engineered core (MDF)
Route for Glass | Not Available
Minimum Size | 3" x 3" minimum (for doors and drawer fronts)
Maximum Size | 48" x 96" maximum, warranted to 31" x 60"

For warranty information on Engineered Doors from Northern Contours, click here

ENGINEERED DOORS ARE AVAILABLE FOR IKEA PROJECTS ONLY

### Slim Stratus

### Slim Mist

### Slim Haze

### Slim Silt

### Slim Gauntlet

### Slim Flint

### Slim Onyx

### Slim Midnight

### Slim Surf

### Slim Denim

### Slim Aloe

### Slim Sage

!
Mobile mode
To create online store ShopFactory eCommerce software was used.